**Introduction:**

List of SAS Airline approved trackers for use when transporting cargo shipments.

**Cargo tracking devices:**

A cargo tracking device is a Portable Electronic Device (PED) attached to or included in airfreight (e.g. in or on containers, pallets or parcels). Cargo tracking devices can be assigned to the category of nonintentional transmitters or T-PEDs.

Non-intentional transmitters can non-intentionally radiate RF transmissions, sometimes referred to as spurious missions. This category includes, but is not limited to, calculators, cameras, radio receivers, audio and video players, electronic games and toys; when these devices are not equipped with a transmitting function.

If the device is a T-PED, it complies with the European Norms (EN) for transmissions.

If you intend to use a tracking device that is not able to send any wireless data then scroll down to the “Approved Data Loggers” section. (Wireless data are data send by wifi, Bluetooth, NFC, NB-LTE, 2G, 3G, 4G and 5G or any other wireless technique).

**Approved trackers:**

|  |  |
| --- | --- |
| **Manufacturer** | **Device (Model Number)** |
| 7PSolution | * GD100 Disposable Single-Use Tracking Device * GL200 tracker with SecureFlight * GL300W tracker with SecureFlight |
| Controlant | * CO 10.01 Real-Time Logger * Controlant Saga Data Logger |
| Emerson | * GO Real-Time Tracker |
| Fastcom | * MicroTAG. |
| FreightWatch | * ILC2000 FlightSmartTM Air Cargo Tracker |
| Intelyt | * Cargo Tracker iTAG-IDC-ITG-V3.3 |
| Key7 | * EPS2 Microtracker |

**Approved trackers(continued):**

|  |  |
| --- | --- |
| **Manufacturer** | **Device (Model Number)** |
| OnAsset Intelligence | * Sentinel 100/100L/100A/100P/100B/100S Cargo Tracking devices * SENTRY 400 FlightSafe * SENTRY 500 FlightSafe |
| Roam Bee | * Roambee Sensor Bee |
| Sendum | * PT300 and PT300D with Advanced Sensor Pack (ASP)   *Note: Basic Sensor Pack (BSP) and Accessory Pack (AP) is NOT approved for transport.* |
| SenseAware | * SenseAware 2000 |
| Sensitech | * TT Geo Ultra Extended, * TT Geo Ultra, * TT Geo Ultra Dry Ice Extended, * TT Geo Ultra Dry Ice * TempTale GEO X (T11013210) * TempTale GEO XE (T11013220) * TempTale GEO XP (T11013230) * TempTale GEO XEP (T11013240) |
| Tive | * TT-7000, * TT-7100 |

**Approved Data Loggers:**

A tracking device that is not able to send any wireless data. Wireless data are data send by Wi-Fi, Bluetooth, NFC, NB-LTE, 2G, 3G, 4G and 5G or any other wireless technique.

If the data logger contains Lithium batteries, IATA Dangerous Goods Regulations applies.

|  |  |
| --- | --- |
| **Manufacturer** | **Device (Model Number)** |
| Berlinger | * Q-tag CLm doc |
| DeltaTrak | * FlashLink Mini PDF In-Transit Logger Models 31010, 31011, 31012 |
| Sensitech | * TempTale Ultra * TempTale (TT) Ultra Bio * TempTale Ultra Probeless Dry Ice Monitor |
| TempSen | * ITAG 3 Pro |

**Document info:**

|  |  |  |
| --- | --- | --- |
| **Author:** | **Approved by:** | **Effective date:** |
| Michael Beck, CPHFD | Michael Beck, CPHFD | 10APR2024 |
| **Document review date:** | **Document review by:** | **Department:** |
| 10APR2024 | Michael Beck, CPHFD | HQSS |
| **SCM Document:** | **sascargo.com:** | **Live Document:** |
| Yes | Yes | Yes |